

Constant motor control signals take higher priority

2. Message sent to take readings

3. Response contains data reading

Slave PIC

ARM

4. Data reading sent to ARM immediately

1. Timer interrupts on Master PIC at maximum frequency for individual sensor device

Master PIC